CN\_LAB-4

Write – up:

1. Configure the topology like in the previous experiments.
2. In the middle router add static address.
3. In the router0 and router 1, add default routes.
   1. 0.0.0.0 0.0.0.0 20.0.0.1
   2. 0.0.0.0 0.0.0.0 30.0.0.2
4. Ping the message

Outcome:

1. When you are not sure about the destination address of a router to configure the next hop address, then use default route settings and configure the routers.